2024/9/17

Install a SHCS M3X8 from the back to secure the main body and spindle and make sure the spindle is free to rotate.

Afterwards the M3X8 screw and spindle can be rotated by an electric screwdriver.

When loading the component tape, use some sticky tape to hold the end of the component tape to the circumference of the spindle.


==================

License: CC BY-NC-SA 4.0

pandaplacer.com