202406014
=============================
Choose of print material:
# PLA/PETG/ABS/:
PPBF-AS2-**-V1.0-All_PLA.3mf

# PETG/ABS:
PPBF-AS2-TopSpring-V1.0.STL
PPBF-AS2-TopClampingPlate_**-V1.0.STL

Choose the color of the material:
Preferably with both black and white color difference, which is compatible with white, black, and clear tapes.
e.g. green, blue, yellow, orange...

* Some edges of the parts are pre-added with BRIM, please use a tool to remove the brim before assembly.
=============================

Assembly Notes:
1. Use the second (outer) mounting hole on the Pandaplacer-A1 frame.
2. Before inserting the SERVO, adjust the SERVO-Arm a bit towards to the retraction direction.
3. All M2X6 adjusting screws have been changed to M3X4 set screws.
4. Using 2 O-rings on the spool and the friction is just right. More can be used when needed.
5. Connecting LockerArm and LockerTnut using M2X16 or M2X14.
6. The mounting position needs to be aligned with the pin heads of the feeder controllers.
7. If necessary, update the feeder controller firmware (for orders purchased on 2023) to support M611 command.

=============================
Change in OpenPnP settings:

Driver>SLFC(feeder controller)>Gcode>

AutoFeeder_Enable > ACTUATE_BOOLEAN_COMMAND >
{True:M610 S1}{False:M611 S0}
{True: M611 S0  }{False: M610 S0}

Modify each of the corresponding XmmAdvance (2/4/8/12...) command:
AutoFeeder_XmmAdvance > ACTUATE_DOUBLE_COMMAND >
M611 N{IntegerValue} S1
M600 N{IntegerValue} FX X1
M611 N{IntegerValue} S0

* FX replaced with actual F2/F4/F8/F12... Corresponds to XmmAdvance command
=============================


License: CC BY-NC-SA 4.0

Pandaplacer.com